# :MEASure:HORizontal:DCYCle:OCCurrences

Duty Cycle Commands

- :MEASure:HORizontal:DCYCle
- :MEASure:HORizontal:DCYCle:EDIRection
- :MEASure:HORizontal:DCYCle:FAVorite
- :MEASure:HORizontal:DCYCle:LOCation?
- :MEASure:HORizontal:DCYCle:OCCurrences
- :MEASure:HORizontal:DCYCle:REGion
- :MEASure:HORizontal:DCYCle:SOURce
- :MEASure:HORizontal:DCYCle:STATus?
- :MEASure:HORizontal:DCYCle:STATus:DETails?
- :MEASure:HORizontal:DCYCle:STATus:REASon?
- :MEASure:HORizontal:DCYCle:UREFerence:STATe
- :MEASure:HORizontal:DCYCle:UREFerence:VALue

## Command Syntax

    :MEASure:HORizontal:DCYCle:OCCurrences  {ONE | ALL}

## Query Syntax

    :MEASure:HORizontal:DCYCle:OCCurrences?

## Description

This command lets you select between Measure One and Measure All in the user interface which specifies whether Infiniium should make one edge-related measurement per acquisition or multiple measurements per acquisition using all edges in the acquisition.

When Measure One is selected:

- Measurements using edges are made on a particular edge (or pair of edges). Measurements are made on the edge closest to the timebase reference (see `:TIMebase:REFerence`).
- Measurement statistics are calculated for the one specific edge only and compiled over a number of acquisitions. A Single acquisition adds a single value to the measurement statistics. All other edges are ignored.

When Measure All is selected:

- Measurements using edges are made on all edges (or all pairs of edges) in the acquisition.

- The "Current" measurement result (see `:MEASure:RESults?`) is taken from the measurement closest to the timebase reference. For measurements on memory waveforms, it is the measurement closest to the horizontal X position setting. Annotations are shown at the "Current" measurement result.

Switching between Measure One and Measure All restarts the measurement count.

## Query Response

    {ONE | ALL}