# :TRIGger:SHOLd:MODE

:TRIGger Setup And Hold Commands

- :TRIGger:SHOLd:DSOurce
- :TRIGger:SHOLd:CSOurce:EDGE
- :TRIGger:SHOLd:CSOurce
- :TRIGger:SHOLd:HTIMe
- :TRIGger:SHOLd:MODE
- :TRIGger:SHOLd:STIMe

## Command Syntax

    :TRIGger:SHOLd:MODE  {STIMe | HTIMe | SOHTime}

## Query Syntax

    :TRIGger:SHOLd:MODE?

## Description

In the Setup And Hold trigger mode (see `:TRIGger:MODE`), this command selects the kind of setup and hold violations to trigger on:

- `STIMe` — Looks for violations where the data signal crosses though the region specified by the `:TRIGger:SHOLd:STIMe` time.
- `HTIMe` — Looks for violations where the data signal crosses through the region specified by the `:TRIGger:SHOLd:HTIMe` time.
- `SOHTime` — Looks for violations where the data signal crosses though the combined region specified by the `:TRIGger:SHOLd:STIMe` time and the `:TRIGger:SHOLd:HTIMe` time.