# :MEASure:LIST:ITEM{N}:OCCurrences

Results Panel List Commands

- :MEASure:LIST:CLEar
- :MEASure:LIST:ITEM{N}:COUNt?
- :MEASure:LIST:ITEM{N}:COUNt:STATus?
- :MEASure:LIST:ITEM{N}:COUNt:STATus:REASon?
- :MEASure:LIST:ITEM{N}:CURRent?
- :MEASure:LIST:ITEM{N}:MAXimum?
- :MEASure:LIST:ITEM{N}:MAXimum:STATus?
- :MEASure:LIST:ITEM{N}:MAXimum:STATus:REASon?
- :MEASure:LIST:ITEM{N}:MEAN?
- :MEASure:LIST:ITEM{N}:MEAN:STATus?
- :MEASure:LIST:ITEM{N}:MEAN:STATus:REASon?
- :MEASure:LIST:ITEM{N}:MINimum?
- :MEASure:LIST:ITEM{N}:MINimum:STATus?
- :MEASure:LIST:ITEM{N}:MINimum:STATus:REASon?
- :MEASure:LIST:ITEM{N}:NAME?
- :MEASure:LIST:ITEM{N}:OCCurrences
- :MEASure:LIST:ITEM{N}:REGion
- :MEASure:LIST:ITEM{N}:SDEViation?
- :MEASure:LIST:ITEM{N}:SDEViation:STATus?
- :MEASure:LIST:ITEM{N}:SDEViation:STATus:REASon?
- :MEASure:LIST:ITEM{N}:SOURce
- :MEASure:LIST:ITEM{N}:STATus?
- :MEASure:LIST:ITEM{N}:STATus:DETails?
- :MEASure:LIST:ITEM{N}:STATus:REASon?
- :MEASure:LIST:MOVE
- :MEASure:LIST:REMove
- :MEASure:LIST:SELect
- :MEASure:RESults?

## Command Syntax

    :MEASure:LIST:ITEM{N}:OCCurrences  {ONE | ALL}

Where {N} is a number from 1 to 64 that identifies a measurement row in the Results table. For example, `ITEM4`.

## Query Syntax

    :MEASure:LIST:ITEM{N}:OCCurrences?

## Description

This command lets you select between Measure One and Measure All in the user interface which specifies whether Infiniium should make one edge-related measurement per acquisition or multiple measurements per acquisition using all edges in the acquisition.

When Measure One is selected:

- Measurements using edges are made on a particular edge (or pair of edges). Measurements are made on the edge closest to the timebase reference (see `:TIMebase:REFerence`).
- Measurement statistics are calculated for the one specific edge only and compiled over a number of acquisitions. A Single acquisition adds a single value to the measurement statistics. All other edges are ignored.

When Measure All is selected:

- Measurements using edges are made on all edges (or all pairs of edges) in the acquisition.
- For Period and Frequency measurements, if the first edge is rising (or falling), pairs of rising (or falling) edges throughout the acquisition are used to make the measurements.

- The "Current" measurement result (see `:MEASure:RESults?`) is taken from the measurement closest to the timebase reference. For measurements on memory waveforms, it is the measurement closest to the horizontal X position setting. Annotations are shown at the "Current" measurement result.

Switching between Measure One and Measure All restarts the measurement count.

## Query Response

    {ONE | ALL}

## Related Commands

- `:MEASure:LIST:CLEar` Clears the results table.
- `:MEASure:LIST:ITEM{N}:REGion` Selects single measurement in the results table.
- `:MEASure:LIST:ITEM{N}:SOURce` Changes the source of an existing measurement in the results table.
- `:MEASure:LIST:MOVE` Moves a measurement from one location to another in the results table.
- `:MEASure:LIST:REMove` Removes single measurement from the results table.
- `:MEASure:LIST:SELect` Selects single measurement in the results table.