# :MEASure:DATA:DRATe:NDRate

Data Rate Commands

- :MEASure:DATA:DRATe
- :MEASure:DATA:DRATe:DWMode
- :MEASure:DATA:DRATe:FAVorite
- :MEASure:DATA:DRATe:LOCation?
- :MEASure:DATA:DRATe:NDRate
- :MEASure:DATA:DRATe:OCCurrences
- :MEASure:DATA:DRATe:REGion
- :MEASure:DATA:DRATe:SOURce
- :MEASure:DATA:DRATe:STATus?
- :MEASure:DATA:DRATe:STATus:DETails?
- :MEASure:DATA:DRATe:STATus:REASon?
- :MEASure:DATA:DRATe:UREFerence:STATe
- :MEASure:DATA:DRATe:UREFerence:VALue

## Command Syntax

    :MEASure:DATA:DRATe:NDRate <nominal_data_rate>

<nominal_data_rate> is a double.

## Query Syntax

    :MEASure:DATA:DRATe:NDRate?

## Description

Sets the global Nominal Data Rate for clock recovery. This is the baud rate associated with the input waveform.