# :CALibrate Probe Commands

:CALibrate Probe Commands

- :CALibrate:PROBe:CHANnel:ENABled
- :CALibrate:PROBe:CHANnel:SKEW:ENABled
- :CALibrate:PROBe:CHANnel:SKEW:STATus?
- :CALibrate:PROBe:CHANnel:SKEW:STATus:DETails?
- :CALibrate:PROBe:CHANnel:SKEW:STATus:DTEMperature?
- :CALibrate:PROBe:CHANnel:SKEW:STATus:TIME?
- :CALibrate:PROBe:CHANnel:STARt
- :CALibrate:PROBe:CHANnel:STATus?
- :CALibrate:PROBe:CHANnel:STATus:DETails?
- :CALibrate:PROBe:CHANnel:STATus:DTEMperature?
- :CALibrate:PROBe:CHANnel:STATus:TIME?
- :CALibrate:PROBe:CHANnel:VERTical:ENABled
- :CALibrate:PROBe:CHANnel:VERTical:STATus?
- :CALibrate:PROBe:CHANnel:VERTical:STATus:DETails?
- :CALibrate:PROBe:CHANnel:VERTical:STATus:DTEMperature?
- :CALibrate:PROBe:CHANnel:VERTical:STATus:TIME?

## To Perform a Probe Calibration

1. Connect a probe.

2. Enable all probe calibrations using `:CALibrate:PROBe:CHANnel:ENABled`, or individual probe calibrations using `:CALibrate:PROBe:CHANnel:VERTical:ENABled` and `:CALibrate:PROBe:CHANnel:SKEW:ENABled`.

   The `ENABled` settings commands specify only which calibrations to run. They do not enable or disable calibrations or default the calibration factors.

3. Use the `:CALibrate:PROBe:CHANnel:STARt` command.