# :MEASure:CLOCk:CTIerror:EDIRection

Clock TIE Commands

- :MEASure:CLOCk:CTIerror
- :MEASure:CLOCk:CTIerror:EDIRection
- :MEASure:CLOCk:CTIerror:FAVorite
- :MEASure:CLOCk:CTIerror:LOCation?
- :MEASure:CLOCk:CTIerror:OCCurrences
- :MEASure:CLOCk:CTIerror:REGion
- :MEASure:CLOCk:CTIerror:SOURce
- :MEASure:CLOCk:CTIerror:STATus?
- :MEASure:CLOCk:CTIerror:STATus:DETails?
- :MEASure:CLOCk:CTIerror:STATus:REASon?
- :MEASure:CLOCk:CTIerror:TIEFilter
- :MEASure:CLOCk:CTIerror:TIEFilter:DFACtor
- :MEASure:CLOCk:CTIerror:TIEFilter:SHAPe
- :MEASure:CLOCk:CTIerror:TIEFilter:STARt
- :MEASure:CLOCk:CTIerror:TIEFilter:STOP
- :MEASure:CLOCk:CTIerror:TIEFilter:TYPE
- :MEASure:CLOCk:CTIerror:UNITs
- :MEASure:CLOCk:CTIerror:UREFerence:STATe
- :MEASure:CLOCk:CTIerror:UREFerence:VALue

## Command Syntax

    :MEASure:CLOCk:CTIerror:EDIRection {RISing | FALLing | BOTH}

## Query Syntax

    :MEASure:CLOCk:CTIerror:EDIRection?

## Description

For the Clock TIE measurement (see `:MEASure:CLOCk:CTIerror`), specifies the waveform's edges to be measured: rising, falling or both edges.

When BOTH is selected, there will be annotations for both the rising edge measurement and the falling edge measurement.

## Example Command Sequence

This sequence sets up the measurement on rising edges only.

    :MEASure:CLOCk:CTIerror:SOURce CHAN1_1
    :MEASure:CLOCk:CTIerror:EDIRection RISing
      //  Perform measurement
    :MEASure:CLOCk:CTIerror
    :MEASure:CLOCk:CTIerror?