# :MEASure:EYE:JITTer:DEFine:UNITs

Eye Jitter Commands

- :MEASure:EYE:JITTer
- :MEASure:EYE:JITTer:DEFine:SIGNal
- :MEASure:EYE:JITTer:DEFine:SIGNal:AUTodetect
- :MEASure:EYE:JITTer:DEFine:UNITs
- :MEASure:EYE:JITTer:FAVorite
- :MEASure:EYE:JITTer:FORMat
- :MEASure:EYE:JITTer:LOCation?
- :MEASure:EYE:JITTer:SOURce
- :MEASure:EYE:JITTer:STATus?
- :MEASure:EYE:JITTer:STATus:DETails?
- :MEASure:EYE:JITTer:STATus:REASon?
- :MEASure:EYE:JITTer:UNITs

## Command Syntax

    :MEASure:EYE:JITTer:DEFine:UNITs {SECond | UINTerval}

## Query Syntax

    :MEASure:EYE:JITTer:DEFine:UNITs?

## Description

Selects measurement units for Jitter values that are reported in the Results table and shown on the x-axis of displayed graphs. Choices are seconds (default value) or Unit Interval (UI), which is the symbol period of the data.