# :LTESt:ACQuire:SIMage:WINDow

:LTESt Acquisition Commands

- :LTESt:ACQuire:CTYPe
- :LTESt:ACQuire:CTYPe:SAMPles
- :LTESt:ACQuire:CTYPe:WAVeforms
- :LTESt:ACQuire:SIMage:FNAMe
- :LTESt:ACQuire:SIMage:FNAMe:AUPDate
- :LTESt:ACQuire:SIMage:FNAMe:USTandard
- :LTESt:ACQuire:SIMage:FTYPe?
- :LTESt:ACQuire:SIMage:IMETadata
- :LTESt:ACQuire:SIMage:INVert
- :LTESt:ACQuire:SIMage:MONochrome
- :LTESt:ACQuire:SIMage:SINClude
- :LTESt:ACQuire:SIMage:STATe
- :LTESt:ACQuire:SIMage:WINDow
- :LTESt:ACQuire:STATe
- :LTESt:ACQuire:SWAVeform:CHANnel{N}:FNAMe
- :LTESt:ACQuire:SWAVeform:CHANnel:FTYPe
- :LTESt:ACQuire:SWAVeform:CHANnel{N}:STATe
- :LTESt:ACQuire:SWAVeform:CHANnel{N}:WMEMory
- :LTESt:ACQuire:SWAVeform:CMODe{N}:FNAMe
- :LTESt:ACQuire:SWAVeform:CMODe:FTYPe
- :LTESt:ACQuire:SWAVeform:CMODe{N}:STATe
- :LTESt:ACQuire:SWAVeform:CMODe{N}:WMEMory WMEMory{1:8}
- :LTESt:ACQuire:SWAVeform:DIFF{N}:FNAMe
- :LTESt:ACQuire:SWAVeform:DIFF:FTYPe
- :LTESt:ACQuire:SWAVeform:DIFF{N}:STATe
- :LTESt:ACQuire:SWAVeform:DIFF{N}:WMEMory
- :LTESt:ACQuire:SWAVeform:FUNCtion{N}:FNAMe
- :LTESt:ACQuire:SWAVeform:FUNCtion{N}:STATe
- :LTESt:ACQuire:SWAVeform:FUNCtion{N}:WMEMory
- :LTESt:ACQuire:SWAVeform:RESet

## Command Syntax

    :LTESt:ACQuire:SIMage:WINDow  {DISPlay | TIME{1} | SHERtz{1:4} | DBHertz{1:4} | DHERtz{1:4}}

## Query Syntax

    :LTESt:ACQuire:SIMage:WINDow?

## Query Response

    {1 | 0}

## Description

When reporting a screen image as a result of an acquisition limit test, use this command to selects which portion of the screen to include in the image. To actually specify that a screen image is saved, use the `:LTESt:ACQuire:SIMage:STATe` command. The following selections are available:

DISPlay
  Includes the entire Infiniium 2026 screen in the captured screen image.
TIMe1
  Includes only the Waveform content window in the captured screen image.
SHERtz{1:4}
  Includes only the Delay 1, Delay 2, Delay 3, or Delay 4 content window in the captured screen image. This selection is only available if one of these windows is actually displayed. Delay windows 2, 3, and 4 can only be displayed programmatically and not using front-panel controls. The group Delay window can be selected as a display output format for FFT functions (`:FUNCtion:FOPerator FFT`).
DBHertz{1:4}
  Includes only the Decibels (Hz) 1, Decibels (Hz) 2, Decibels (Hz) 3, or Decibels (Hz) 4 content window in the captured screen image. This selection is only available if one of these windows is actually displayed. Decibels (Hz) windows 2, 3, and 4 can only be displayed programmatically and not using front-panel controls. The group Decibels (Hz) window can be selected as a display output format for FFT functions (`:FUNCtion:FOPerator FFT`).
DHERtz{1:4}
  Includes only the Degrees (Hz) 1, Degrees (Hz) 2, Degrees (Hz) 3, or Degrees (Hz) 4 content window in the captured screen image. This selection is only available if one of these windows is actually displayed. Degrees (Hz) windows 2, 3, and 4 can only be displayed programmatically and not using front-panel controls. The group Degrees (Hz) window can be selected as a display output format for FFT functions (`:FUNCtion:FOPerator FFT`).