# :CALibrate:PROBe:CHANnel:SKEW:STATus:DETails?

:CALibrate Probe Commands

- :CALibrate:PROBe:CHANnel:ENABled
- :CALibrate:PROBe:CHANnel:SKEW:ENABled
- :CALibrate:PROBe:CHANnel:SKEW:STATus?
- :CALibrate:PROBe:CHANnel:SKEW:STATus:DETails?
- :CALibrate:PROBe:CHANnel:SKEW:STATus:DTEMperature?
- :CALibrate:PROBe:CHANnel:SKEW:STATus:TIME?
- :CALibrate:PROBe:CHANnel:STARt
- :CALibrate:PROBe:CHANnel:STATus?
- :CALibrate:PROBe:CHANnel:STATus:DETails?
- :CALibrate:PROBe:CHANnel:STATus:DTEMperature?
- :CALibrate:PROBe:CHANnel:STATus:TIME?
- :CALibrate:PROBe:CHANnel:VERTical:ENABled
- :CALibrate:PROBe:CHANnel:VERTical:STATus?
- :CALibrate:PROBe:CHANnel:VERTical:STATus:DETails?
- :CALibrate:PROBe:CHANnel:VERTical:STATus:DTEMperature?
- :CALibrate:PROBe:CHANnel:VERTical:STATus:TIME?

## Query Syntax

    :CALibrate:PROBe:CHANnelN:SKEW:STATus:DETails?

Where N identifies a specific channel in the form "<connection1-8>_<ch1-8>". With connection 1, the connection number part (that is, "1_") is optional, and you can simply use the channel number "<ch1-8>". For example, connection 4 channel 2 is `CHANnel4_2`.

## Description

Queries a string of status details for the Skew Adjustment status for the probe on the specified channel.

## Parent Command

- `:CALibrate:PROBe:CHANnel:SKEW:STATus?`