# PAM Measurements

Subtopics

- PAM Rise/Fall Times
- PAM Levels RMS
- PAM Levels
- PAM Levels
- PAM Levels RMS
- PAM Levels Peak-Peak
- PAM Level Skews
- PAM Eye Levels
- PAM Eye Skews
- PAM VEC
- PAM Eye Heights
- PAM Eye Widths
- PAM Overshoot
- PAM Undershoot
- PAM Eye Linearity
- PAM Pk-Pk Amplitude

If the PAM-N Analysis software option is installed, you can make the following measurements on PAM waveforms.

The Linearity, Levels, and Levels RMS measurements can also be used on NRZ waveforms (0 and 1 levels for one eye, in other words, PAM-2).

- PAM-N Analysis

## Toolbar 1 of 3

Rise/Fall Times
Levels
Levels RMS
Levels
Levels RMS
Levels Peak-Peak

## Toolbar 2 of 3

Level Skews
Eye Levels
Eye Skews
Vertical Eye Closure
Eye Heights
Eye Widths

## Toolbar 3 of 3

PAM Overshoot
PAM Undershoot
Linearity
Pk-Pk Amplitude