# :MEASure:HORizontal:TEDGe:EDIRection

Time-at-Edge Commands

- :MEASure:HORizontal:TEDGe
- :MEASure:HORizontal:TEDGe:EDIRection
- :MEASure:HORizontal:TEDGe:FAVorite
- :MEASure:HORizontal:TEDGe:LOCation?
- :MEASure:HORizontal:TEDGe:NUMBer
- :MEASure:HORizontal:TEDGe:REGion
- :MEASure:HORizontal:TEDGe:SOURce
- :MEASure:HORizontal:TEDGe:STATus?
- :MEASure:HORizontal:TEDGe:STATus:DETails?
- :MEASure:HORizontal:TEDGe:STATus:REASon?
- :MEASure:HORizontal:TEDGe:THReshold
- :MEASure:HORizontal:TEDGe:UREFerence:STATe
- :MEASure:HORizontal:TEDGe:UREFerence:VALue

## Command Syntax

    :MEASure:HORizontal:TEDGe:EDIRection  {RISing | FALLing}

## Query Syntax

    :MEASure:HORizontal:TEDGe:EDIRection?

## Description

For the Time-at-Edge measurement, specifies the edge direction used to identify the waveform's edge: rising or falling. To specify the edge number, use the `:MEASure:HORizontal:TEDGe:NUMBer` command. To specify the edge threshold, use the `:MEASure:HORizontal:TEDGe:THReshold` command.

## Example Command Sequence

    :MEASure:HORizontal:TEDGe:SOURce CHAN2_2
    :MEASure:HORizontal:TEDGe:EDIRection RISing
    :MEASure:HORizontal:TEDGe:NUMBer 2
    :MEASure:HORizontal:TEDGe:THReshold MIDDle
    :MEASure:HORizontal:TEDGe
    :MEASure:HORizontal:TEDGe?