# :TRIGger:CHANnel:LEVel

:TRIGger General Commands

- :TRIGger:AUX:LEVel
- :TRIGger:AUX:LEVel:FIFTy
- :TRIGger:CHANnel:HTHReshold
- :TRIGger:CHANnel:LEVel
- :TRIGger:CHANnel:LEVel:FIFTy
- :TRIGger:CHANnel:LTHReshold
- :TRIGger:FORCe
- :TRIGger:HYSTeresis
- :TRIGger:MODE
- :TRIGger:SWEep

## Command Syntax

    :TRIGger:CHANnelN:LEVel <level>

Where N identifies a specific channel in the form "<connection1-8>_<ch1-8>". With connection 1, the connection number part (that is, "1_") is optional, and you can simply use the channel number "<ch1-8>". For example, connection 4 channel 2 is `CHANnel4_2`.

<level> is a double.

## Query Syntax

    :TRIGger:CHANnelN:LEVel?

## Description

Specifies the trigger level for a particular analog channel input. This is the threshold level that the signal must cross to trigger on the signal.

The trigger level can be adjusted in all trigger modes (`:TRIGger:MODE`). However, note that some trigger modes have lower and upper thresholds; in these cases, the `:TRIGger:CHANnel:LEVel` command maps to the upper threshold (see `:TRIGger:CHANnel:HTHReshold`).