# :TRIGger:QUALify:ZONE:ZONE{N}:SOURce

:TRIGger Qualify Commands

- :TRIGger:QUALify:FOQualify
- :TRIGger:QUALify:MEASure:LLIMit
- :TRIGger:QUALify:MEASure:LOCation
- :TRIGger:QUALify:MEASure:REGion
- :TRIGger:QUALify:MEASure:ULIMit
- :TRIGger:QUALify:MODE
- :TRIGger:QUALify:STATe
- :TRIGger:QUALify:ZONE:ISZLogic
- :TRIGger:QUALify:ZONE:ZONE{N}:LOGic
- :TRIGger:QUALify:ZONE:ZONE{N}:SOURce
- :TRIGger:QUALify:ZONE:ZONE{N}:STATe
- :TRIGger:QUALify:ZONE:ZONE{N}:X
- :TRIGger:QUALify:ZONE:ZONE{N}:Y

## Command Syntax

    :TRIGger:QUALify:ZONE:ZONEN:SOURce  <waveform_source>

Where N identifies one of eight possible zones {1:8}. For example, `ZONE2`.

Where <waveform_source> can be one of the following:

- `CHANnel{N}`

  Where N identifies a specific channel in the form "<connection1-8>_<ch1-8>". With connection 1, the connection number part (that is, "1_") is optional, and you can simply use the channel number "<ch1-8>". For example, connection 4 channel 2 is `CHANnel4_2`..

- `CMODe{N}`

  Where N identifies a specific common-mode waveform in the form "<connection1-8>_<ch1|ch3|ch5|ch7>". With connection 1, the connection number part (that is, "1_") is optional, and you can simply use the channel number "<ch1|ch3|ch5|ch7>". When two channels are paired to create a differential waveform and a common-mode waveform, the odd-numbered channel is used when specifying the waveform. For example, connection 5 common-mode waveform 3 (from the pairing of channels 3 and 4) is `CMODe5_3`.

- `DIFF{N}>`

  Where N identifies a specific differential waveform in the form "<connection1-8>_<ch1|ch3|ch5|ch7>". With connection 1, the connection number part (that is, "1_") is optional, and you can simply use the channel number "<ch1|ch3|ch5|ch7>". When two channels are paired to create a differential waveform and a common-mode waveform, the odd-numbered channel is used when specifying the waveform. For example, connection 5 differential waveform 3 (from the pairing of channels 3 and 4) is `DIFF5_3`.

## Query Syntax

    :TRIGger:QUALify:ZONE:ZONEN:SOURce?

## Description

Specifies the signal on which the zone operates.