# :CMODe:SNDRatio:SAVE

:CMODe SNDR Setup Commands

- :CMODe:SNDRatio:FILE:NAME
- :CMODe:SNDRatio:FILE:RELoad
- :CMODe:SNDRatio:LFPDelay
- :CMODe:SNDRatio:LFPLength
- :CMODe:SNDRatio:NAVerages
- :CMODe:SNDRatio:PUINterval
- :CMODe:SNDRatio:RLMStandard
- :CMODe:SNDRatio:RNComp
- :CMODe:SNDRatio:RNCValue:LEVel
- :CMODe:SNDRatio:SAVE
- :CMODe:SNDRatio:SAVE:FILE
- :CMODe:SNDRatio:STANdard

## Command Syntax

    :CMODeN:SNDRatio:SAVE {OFF | ON}

Where N identifies a specific common-mode waveform in the form "<connection1-8>_<ch1|ch3|ch5|ch7>". With connection 1, the connection number part (that is, "1_") is optional, and you can simply use the channel number "<ch1|ch3|ch5|ch7>". When two channels are paired to create a differential waveform and a common-mode waveform, the odd-numbered channel is used when specifying the waveform. For example, connection 5 common-mode waveform 3 (from the pairing of channels 3 and 4) is `CMODe5_3`.

## Query Syntax

    :CMODeN:SNDRatio:SAVE?

## Description

When `AUTomatic` is selected as the SNDR standard (see `:CMODe:SNDRatio:STANdard`), this command lets you turn on or off saving of the automatically calculated Sigma-n locations to a standard definition file.

When saving the automatic calculations to a standards file is turned on, use the `:CMODe:SNDRatio:SAVE:FILE` command to specify the file name.