# :WAVeform:CGRade:STATus?

:WAVeform CGRade Commands

- :WAVeform:CGRade:ASCii:DATA?
- :WAVeform:CGRade:COLumns?
- :WAVeform:CGRade:INTeger:DATA?
- :WAVeform:CGRade:POINts?
- :WAVeform:CGRade:ROWS?
- :WAVeform:CGRade:STATus?
- :WAVeform:CGRade:STATus:REASon?
- :WAVeform:CGRade:UICount?
- :WAVeform:CGRade:WCOunt?
- :WAVeform:CGRade:XINCrement?
- :WAVeform:CGRade:XML:READ?
- :WAVeform:CGRade:XML:WRITe?
- :WAVeform:CGRade:XORigin?
- :WAVeform:CGRade:YINCrement?
- :WAVeform:CGRade:YORigin?

## Query Syntax

    :WAVeform:CGRade:STATus?

## Description

Queries the status of the color-grade gray-scale waveform data and returns the strings shown in the following table. Use the `:WAVeform:CGRade:STATus:REASon?` child query to return a string that indicates why the data is invalid or questionable.

STATus? Query Response
Response | Description
--- | ---
CORR | The waveform data is correct.
INV | The waveform data is invalid. Check to see if eye diagram data is displayed on the screen.
QUES | The waveform data is questionable. Confirm that the eye diagram data is not clipped high, clipped low, or has holes.

Query the data using one of the following two commands:

- :WAVeform:CGRade:ASCii:DATA?
- :WAVeform:CGRade:INTeger:DATA?

## Child Commands

- `:WAVeform:CGRade:STATus:REASon?`