# :MEASure:HORizontal:PCOunt:UREFerence:VALue

Pulse Count Commands

- :MEASure:HORizontal:PCOunt
- :MEASure:HORizontal:PCOunt:FAVorite
- :MEASure:HORizontal:PCOunt:LOCation?
- :MEASure:HORizontal:PCOunt:PTYPe
- :MEASure:HORizontal:PCOunt:REGion
- :MEASure:HORizontal:PCOunt:SOURce
- :MEASure:HORizontal:PCOunt:STATus?
- :MEASure:HORizontal:PCOunt:STATus:DETails?
- :MEASure:HORizontal:PCOunt:STATus:REASon?
- :MEASure:HORizontal:PCOunt:UREFerence:STATe
- :MEASure:HORizontal:PCOunt:UREFerence:VALue

## Command Syntax

    :MEASure:HORizontal:PCOunt:UREFerence:VALue <time_location>

<time_location> is a double.

## Query Syntax

    :MEASure:HORizontal:PCOunt:UREFerence:VALue?

## Description

When a user-defined horizontal reference location is enabled (see `:MEASure:HORizontal:PCOunt:UREFerence:STATe`), this command specifies its time location with respect to the trigger (t = 0) location.