# :DISPlay:WINDow:DHERtz{N}:TSIGnal

:DISPlay Freq Domain Windows Commands

- :DISPlay:WINDow:DBHertz{N}:DMODe
- :DISPlay:WINDow:DBHertz{N}:LEGend:EXPand
- :DISPlay:WINDow:DBHertz{N}:LOCation
- :DISPlay:WINDow:DBHertz{N}:TOPMost
- :DISPlay:WINDow:DBHertz{N}:TSIGnal
- :DISPlay:WINDow:DHERtz{N}:DMODe
- :DISPlay:WINDow:DHERtz{N}:LEGend:EXPand
- :DISPlay:WINDow:DHERtz{N}:LOCation
- :DISPlay:WINDow:DHERtz{N}:TOPMost
- :DISPlay:WINDow:DHERtz{N}:TSIGnal
- :DISPlay:WINDow:SHERtz{N}:DMODe
- :DISPlay:WINDow:SHERtz{N}:LEGend:EXPand
- :DISPlay:WINDow:SHERtz{N}:LOCation
- :DISPlay:WINDow:SHERtz{N}:TOPMost
- :DISPlay:WINDow:SHERtz{N}:TSIGnal

## Command Syntax

    :DISPlay:WINDow:DHERtz{N}:TSIGnal  {FUNCtion{1:64} | TRACe{1:128} }

{N} identifies a widow {1:4}.

## Query Syntax

    :DISPlay:WINDow:DHERtz{1:4}:TSIGnal?

## Description

When a Degrees (Hz) waveform content window is displayed in overlapped mode and there are multiple displayed waveforms, selects a waveform to "bring to front" in the graticule area. The output of the FFT function (FFT command) can be defined as phase.

## Sibling Commands

- `:DISPlay:WINDow:DHERtz{N}:DMODe`
- `:DISPlay:WINDow:DHERtz{N}:LEGend:EXPand`
- `:DISPlay:WINDow:DHERtz{N}:LOCation`