# :MEASure:EYE:JITTer:DEFine:SIGNal:AUTodetect

Eye Jitter Commands

- :MEASure:EYE:JITTer
- :MEASure:EYE:JITTer:DEFine:SIGNal
- :MEASure:EYE:JITTer:DEFine:SIGNal:AUTodetect
- :MEASure:EYE:JITTer:DEFine:UNITs
- :MEASure:EYE:JITTer:FAVorite
- :MEASure:EYE:JITTer:FORMat
- :MEASure:EYE:JITTer:LOCation?
- :MEASure:EYE:JITTer:SOURce
- :MEASure:EYE:JITTer:STATus?
- :MEASure:EYE:JITTer:STATus:DETails?
- :MEASure:EYE:JITTer:STATus:REASon?
- :MEASure:EYE:JITTer:UNITs

## Command Syntax

    :MEASure:EYE:JITTer:DEFine:SIGNal:AUTodetect {{ON | 1} | {OFF | 0}}

## Query Syntax

    :MEASure:EYE:JITTer:DEFine:SIGNal:AUTodetect?

## Query Response

    {1 | 0}

## Description

Selects to automatically detect the type of input signal: data or clock. The default is autodetection (`ON`). If a poorly-defined signal cannot be automatically detected, turn off automatic detection specify the signal type with the `:MEASure:EYE:JITTer:DEFine:SIGNal` command.