# :MEASure:EYE:PAM:LEVel:LEVel

Eye Levels Commands

- :MEASure:EYE:PAM:LEVel
- :MEASure:EYE:PAM:LEVel:FAVorite
- :MEASure:EYE:PAM:LEVel:LEVel
- :MEASure:EYE:PAM:LEVel:LOCation?
- :MEASure:EYE:PAM:LEVel:SOURce
- :MEASure:EYE:PAM:LEVel:STATus?
- :MEASure:EYE:PAM:LEVel:STATus:DETails?
- :MEASure:EYE:PAM:LEVel:STATus:REASon?

## Command Syntax

    :MEASure:EYE:PAM:LEVel:LEVel {LEVel0 | LEVel1 | LEVel2 | LEVel3}

## Query Syntax

    :MEASure:EYE:PAM:LEVel:LEVel?

## Description

Selects the eye diagram's level on which to perform the `:MEASure:EYE:PAM:LEVel` measurement. The `LEVel2` argument applies to PAM3 and PAM4 signals. The `LEVel3` argument applies only to PAM4 signals. If you experience difficulties measuring a PAM signal, confirm that the signal-type setting is set appropriately using the `:CHANnel:SIGNal:TYPE` command.

NRZ Waveform
PAM3 Waveform
PAM4 Waveform