# :LTESt:MTESt:SIMage:INVert

:LTESt Mask Limit Commands

- :LTESt:MTESt:MRESult{N}:CTYPe
- :LTESt:MTESt:MRESult{N}:CTYPe:UINTervals
- :LTESt:MTESt:MRESult{N}:CTYPe:WAVeforms
- :LTESt:MTESt:MRESult{N}:SOFailure
- :LTESt:MTESt:MRESult{N}:STATe
- :LTESt:MTESt:SIMage:FNAMe
- :LTESt:MTESt:SIMage:FNAMe:AUPDate
- :LTESt:MTESt:SIMage:FNAMe:USTandard
- :LTESt:MTESt:SIMage:FTYPe?
- :LTESt:MTESt:SIMage:IMETadata
- :LTESt:MTESt:SIMage:INVert
- :LTESt:MTESt:SIMage:MONochrome
- :LTESt:MTESt:SIMage:SINClude
- :LTESt:MTESt:SIMage:STATe
- :LTESt:MTESt:SIMage:WINDow
- :LTESt:MTESt:SWAVeform:CHANnel{N}:FNAMe
- :LTESt:MTESt:SWAVeform:CHANnel:FTYPe
- :LTESt:MTESt:SWAVeform:CHANnel{N}:STATe
- :LTESt:MTESt:SWAVeform:CHANnel{N}:WMEMory
- :LTESt:MTESt:SWAVeform:CMODe{N}:FNAMe
- :LTESt:MTESt:SWAVeform:CMODe:FTYPe
- :LTESt:MTESt:SWAVeform:CMODe{N}:STATe
- :LTESt:MTESt:SWAVeform:CMODe{N}:WMEMory
- :LTESt:MTESt:SWAVeform:DIFF{N}:FNAMe
- :LTESt:MTESt:SWAVeform:DIFF:FTYPe
- :LTESt:MTESt:SWAVeform:DIFF{N}:STATe
- :LTESt:MTESt:SWAVeform:DIFF{N}:WMEMory
- :LTESt:MTESt:SWAVeform:FUNCtion{N}:FNAMe
- :LTESt:MTESt:SWAVeform:FUNCtion{N}:STATe
- :LTESt:MTESt:SWAVeform:FUNCtion{N}:WMEMory
- :LTESt:MTESt:SWAVeform:RESet

## Command Syntax

    :LTESt:MTESt:SIMage:INVert {ON | OFF | 1 | 0}

## Query Syntax

    :LTESt:MTESt:SIMage:INVert?

## Query Response

    {1 | 0}

## Description

Turns on and off the inversion of the graticule area's background color when reporting a screen capture for a mask limit test. When on, an inverted image will be captured and saved into a file by the `:LTESt:MTESt:SIMage:FNAMe` command. The entire application window is saved with the graticule black upon a white background. The waveform colors remain unchanged. When printing a hard copy of the waveform, combined this combine with the `:LTESt:MTESt:SIMage:WINDow` command (graticule only) to save ink or toner. Use the `:LTESt:MTESt:SIMage:FNAMe` command to enable and disable screen-capture reporting. To enable or disable mask limit tests, use the `:LTESt:MTESt:MRESult{N}:STATe` command.