# :MEASure:CLOCk:CTIerror:STATus:REASon?

Clock TIE Commands

- :MEASure:CLOCk:CTIerror
- :MEASure:CLOCk:CTIerror:EDIRection
- :MEASure:CLOCk:CTIerror:FAVorite
- :MEASure:CLOCk:CTIerror:LOCation?
- :MEASure:CLOCk:CTIerror:OCCurrences
- :MEASure:CLOCk:CTIerror:REGion
- :MEASure:CLOCk:CTIerror:SOURce
- :MEASure:CLOCk:CTIerror:STATus?
- :MEASure:CLOCk:CTIerror:STATus:DETails?
- :MEASure:CLOCk:CTIerror:STATus:REASon?
- :MEASure:CLOCk:CTIerror:TIEFilter
- :MEASure:CLOCk:CTIerror:TIEFilter:DFACtor
- :MEASure:CLOCk:CTIerror:TIEFilter:SHAPe
- :MEASure:CLOCk:CTIerror:TIEFilter:STARt
- :MEASure:CLOCk:CTIerror:TIEFilter:STOP
- :MEASure:CLOCk:CTIerror:TIEFilter:TYPE
- :MEASure:CLOCk:CTIerror:UNITs
- :MEASure:CLOCk:CTIerror:UREFerence:STATe
- :MEASure:CLOCk:CTIerror:UREFerence:VALue

## Query Syntax

    :MEASure:CLOCk:CTIerror:STATus:REASon?

## Query Response

Refer to the table "Common Reasons for INV or QUES Status".

## Description

Returns a string that explains the reason for a failed `:MEASure:CLOCk:CTIerror` measurement. If the measurement was successful, a null string is returned.

Additional information about the failure may be available using the `:MEASure:CLOCk:CTIerror:STATus:DETails?` sibling query. Use the `:MEASure:CLOCk:CTIerror:STATus?` parent query to determine if the measurement has failed.

## See Also

- Measurement Errors