# :CMODe:EYE:CURSor

:CMODe EYE Commands

- :CMODe EYE Commands
- :CMODe:EYE:BITS
- :CMODe:EYE:CCOunt
- :CMODe:EYE:CURSor
- :CMODe:EYE:CWINdow
- :CMODe:EYE:DISPlay
- :CMODe:EYE:PATTern
- :CMODe:EYE:UIXPosition
- :CMODe:EYE:UIXRange
- :CMODe:EYE:UUNits
- :CMODe:EYE:WINDow:COPY
- :CMODe:EYE:WINDow:LEFT
- :CMODe:EYE:WINDow:METHod
- :CMODe:EYE:WINDow:RIGHt
- :CMODe:EYE:WINDow:TRACking
- :CMODe:EYE:WINDow:WIDTh
- :CMODe:EYE:XPOSition
- :CMODe:EYE:XSCale

## Command Syntax

    :CMODeN:EYE:CURSor <symbol_0_position>

Where N identifies a specific common-mode waveform in the form "<connection1-8>_<ch1|ch3|ch5|ch7>". With connection 1, the connection number part (that is, "1_") is optional, and you can simply use the channel number "<ch1|ch3|ch5|ch7>". When two channels are paired to create a differential waveform and a common-mode waveform, the odd-numbered channel is used when specifying the waveform. For example, connection 5 common-mode waveform 3 (from the pairing of channels 3 and 4) is `CMODe5_3`.

<symbol_0_position> is an integer from 0 to 15.

## Query Syntax

    :CMODeN:EYE:CURSor?

## Description

When qualifying a real-time eye with symbols in a 16-character pattern (see `:CMODe:EYE:BITS`), this command selects the position of symbol 0 in the pattern. Depending on which position you select for symbol 0, the pattern can include symbols before, after, or both before and after symbol 0. Position 0 means all symbols in the pattern are before symbol 0. Position 15 means all symbols in the pattern are after symbol 0.

To specify the pattern, see the `:CMODe:EYE:PATTern` command.