# :MEASure:EYE:PAM:LINearity:DEFinition

Eye Linearity Commands

- :MEASure:EYE:PAM:LINearity
- :MEASure:EYE:PAM:LINearity:DEFinition
- :MEASure:EYE:PAM:LINearity:FAVorite
- :MEASure:EYE:PAM:LINearity:LOCation?
- :MEASure:EYE:PAM:LINearity:SOURce
- :MEASure:EYE:PAM:LINearity:STATus?
- :MEASure:EYE:PAM:LINearity:STATus:DETails?
- :MEASure:EYE:PAM:LINearity:STATus:REASon?

## Command Syntax

    :MEASure:EYE:PAM:LINearity:DEFinition {RLMA120 | RLMC94 | EYE}

## Query Syntax

    :MEASure:EYE:PAM:LINearity:DEFinition?

## Query Response

     {RLMA120 | RLMC94 | EYE}

## Description

Selects the algorithm used to measure RML (Ratio Level Mismatch) linearity on a PAM signal. The selection arguments are:

RLMA120
  Selects RML based upon IEEE 802.3 Annex 120D.
RLMC94
  Selects RML based upon IEEE 802.3 Clause 94. This is the default setting.
EYE
  Selects Eye Linearity based upon CEI.

The default value is unknown.