# :MEASure:PAM:AMPLitude:UNITs

PAM Analysis Setup Commands

- :MEASure:PAM:AMPLitude:UNITs
- :MEASure:PAM:EYE:ELMethod
- :MEASure:PAM:EYE:ESTiming
- :MEASure:PAM:EYE:PPERcent
- :MEASure:PAM:EYE:TIME:LTDefinition
- :MEASure:PAM:EYE:TIME:UNITs

## Command Syntax

    :MEASure:PAM:AMPLitude:UNITs {AMPLitude | PERCent}

## Description

Sets the amplitude units for PAM level and level RMS (thickness) measurements. The selections are amplitude (volts or Watts) or percent. The following measurements are affected by this setting:

- PAM Eye Levels (`:MEASure:EYE:PAM:LEVel`)
- PAM Eye Levels RMS (`:MEASure:EYE:PAM:RMS`)
- PAM Eye Levels (`:MEASure:EYE:PAM:ELEVel`)
- PAM Eye Heights (`:MEASure:EYE:PAM:EHEight`)
- PAM Levels (`:MEASure:PAM:LEVel`)
- PAM Levels RMS (`:MEASure:PAM:RMS`)

To select the units for Jitter measurements (seconds or unit interval), use the `:MEASure:JITTer:JITTer:UNITs` command.