# :MEASure:EYE:EWIDth:THReshold

NRZ Eye Width Commands

- :MEASure:EYE:EWIDth
- :MEASure:EYE:EWIDth:ALGorithm
- :MEASure:EYE:EWIDth:FAVorite
- :MEASure:EYE:EWIDth:FORMat
- :MEASure:EYE:EWIDth:LOCation?
- :MEASure:EYE:EWIDth:SOURce
- :MEASure:EYE:EWIDth:STATus?
- :MEASure:EYE:EWIDth:STATus:DETails?
- :MEASure:EYE:EWIDth:STATus:REASon?
- :MEASure:EYE:EWIDth:THReshold

## Command Syntax

    :MEASure:EYE:EWIDth:THReshold  {AUTomatic | MTHResholds}

## Query Syntax

    :MEASure:EYE:EWIDth:THReshold?

## Description

Selects the threshold determination method used for the `:MEASure:EYE:EWIDth` measurement.

- `AUTomatic` — Eye Widths are measured at the widest point of the eye crossings. This measurement may be inaccurate if excessive jitter causes difficulty determining the eye crossing.

- `MTHResholds` — Eye Widths are measured at the measurement threshold voltage level that you specified in the Configure Measurements dialog box. This threshold may have been automatically calculated (see `:MEASure:THReshold:GENeral:METHod`).

Specify the threshold determination method before turning the measurement on.