# :MEASure:EYE:PAM:PPAMplitude:STATus:DETails?

:PAM Pk-Pk Amplitude Commands

- :MEASure:EYE:PAM:PPAMplitude
- :MEASure:EYE:PAM:PPAMplitude:FAVorite
- :MEASure:EYE:PAM:PPAMplitude:LOCation?
- :MEASure:EYE:PAM:PPAMplitude:SOURce
- :MEASure:EYE:PAM:PPAMplitude:STATus?
- :MEASure:EYE:PAM:PPAMplitude:STATus:DETails?
- :MEASure:EYE:PAM:PPAMplitude:STATus:REASon?
- :MEASure:EYE:PAM:PPAMplitude:THRatio
- :MEASure:EYE:PAM:PPAMplitude:UNITs

## Query Syntax

    :MEASure:EYE:PAM:PPAMplitude:STATus:DETails?

## Description

Returns a string that may provide additional details for a failed `:MEASure:EYE:PAM:PPAMplitude` measurement. If the measurement was successful, a null string is returned.

For a basic description of a measurement failure, use the `:MEASure:EYE:PAM:PPAMplitude:STATus:REASon?`. Use the `:MEASure:EYE:PAM:PPAMplitude:STATus?` parent query to determine if the measurement has failed.

## See Also

- Measurement Errors