# :MEASure:VERTical:PPHRatio:STATus?

Peak-to-Peak at Hit Ratio Commands

- :MEASure:VERTical:PPHRatio
- :MEASure:VERTical:PPHRatio:FAVorite
- :MEASure:VERTical:PPHRatio:LOCation?
- :MEASure:VERTical:PPHRatio:REGion
- :MEASure:VERTical:PPHRatio:SOURce
- :MEASure:VERTical:PPHRatio:STATus?
- :MEASure:VERTical:PPHRatio:STATus:DETails?
- :MEASure:VERTical:PPHRatio:STATus:REASon?
- :MEASure:VERTical:PPHRatio:THRatio
- :MEASure:VERTical:PPHRatio:UNITs
- :MEASure:VERTical:PPHRatio:UREFerence:STATe
- :MEASure:VERTical:PPHRatio:UREFerence:VALue

## Query Syntax

    :MEASure:VERTical:PPHRatio:STATus?

## Query Response

    {CORR | INV | QUES}

CORR
  The measurement result is correct.
INV
  The measurement result is invalid. A question mark (?) is shown in the displayed results table instead of a measurement result.
QUES
  The measurement result is questionable. A question mark (?) is shown in the displayed results table next to the measurement result.

## Description

Queries the status of the Peak-Peak at Hit Ratio measurement (`:MEASure:VERTical:PPHRatio`). Use the `:MEASure:VERTical:PPHRatio:STATus:REASon?` child query to determine the reason for an invalid or questionable measurement. Additional information about the failure may be available using the `:MEASure:VERTical:PPHRatio:STATus:DETails?` child query.

## See Also

- Measurement Errors

## Measurement Identification

Avoid subtle programming errors! To ensure that the correct measurement is installed or queried, always explicitly identify a measurement when installing a measurement or querying a measured value, status, or detail. To identify a measurement, specify the measurement's source waveform (`:SOURce` child command). With some measurements, you may also need to specify other identifying values. Generally, when selecting a measurement using Infiniium's GUI, if a dialog appears prompting you to select values, you should explicitly specify these values when remotely identifying the measurement.

For example, to return the status of the `:MEASure:VERTical:PPHRatio` measurement:

    Infiniium.write(':MEASure:VERTical:PPHRatio:SOURce CHAN1_1')
    if Infiniium.query(':MEASure:VERTical:PPHRatio:STATus?') == 'CORR';
        measurement = Infiniium.query(':MEASure:VERTical:PPHRatio?')