# :MEASure:JITTer:NOISe:UNITs

Noise Setup Commands

- :MEASure:JITTer:NOISe:ANALysis
- :MEASure:JITTer:NOISe:ERNValue:LEVel
- :MEASure:JITTer:NOISe:MLOCation
- :MEASure:JITTer:NOISe:RNBandwidth
- :MEASure:JITTer:NOISe:RNComp
- :MEASure:JITTer:NOISe:RNCValue:LEVel
- :MEASure:JITTer:NOISe:RNSTabilize
- :MEASure:JITTer:NOISe:RNSValue:LEVel
- :MEASure:JITTer:NOISe:UNITs

## Command Syntax

    :MEASure:JITTerN:NOISe:UNITs {VOLT | UAMPlitude}

Where N identifies one of four possible jitter/noise analyses {1:4}. For example, `JITTer4`.

## Query Syntax

    :MEASure:JITTerN:NOISe:UNITs?

## Description

Selects whether to express measurement values in Volts (V) or Unit Amplitude (UA).