# :NETWorks:TRACe:THReshold:GENeral:AUTO

:NETWorks:TRACe Threshold Commands

- :NETWorks:TRACe:TBASe:GENeral:METHod
- :NETWorks:TRACe:TBASe:RFALl:METHod
- :NETWorks:TRACe:THReshold:GENeral:AUTO
- :NETWorks:TRACe:THReshold:GENeral:BASE
- :NETWorks:TRACe:THReshold:GENeral:HYSTeresis
- :NETWorks:TRACe:THReshold:GENeral:LOWer
- :NETWorks:TRACe:THReshold:GENeral:METHod
- :NETWorks:TRACe:THReshold:GENeral:MIDDle
- :NETWorks:TRACe:THReshold:GENeral:PLOWer
- :NETWorks:TRACe:THReshold:GENeral:PMIDdle
- :NETWorks:TRACe:THReshold:GENeral:PUPPer
- :NETWorks:TRACe:THReshold:GENeral:STZero
- :NETWorks:TRACe:THReshold:GENeral:TOP
- :NETWorks:TRACe:THReshold:GENeral:TRACking
- :NETWorks:TRACe:THReshold:GENeral:UPPer
- :NETWorks:TRACe:THReshold:RFALl:BASE
- :NETWorks:TRACe:THReshold:RFALl:LOWer
- :NETWorks:TRACe:THReshold:RFALl:METHod
- :NETWorks:TRACe:THReshold:RFALl:PLOWer
- :NETWorks:TRACe:THReshold:RFALl:PUPPer
- :NETWorks:TRACe:THReshold:RFALl:TOP
- :NETWorks:TRACe:THReshold:RFALl:TRACking
- :NETWorks:TRACe:THReshold:RFALl:UPPer

## Command Syntax

    :NETWorks:TRACeN:THReshold:GENeral:AUTO

Where N identifies a specific trace and must be selected from 1 to 128 {1:128}.

## Description

When you select the ± Hysteresis threshold definition for the selected signal (see `:NETWorks:TRACe:THReshold:GENeral:METHod`), you can send `:NETWorks:TRACe:THReshold:GENeral:AUTO` to automatically set the Center Threshold (`:NETWorks:TRACe:THReshold:GENeral:MIDDle`) to be halfway between Vmin and Vmax and the Hysteresis value (`:NETWorks:TRACe:THReshold:GENeral:HYSTeresis`) to be ±0.05(Vmax - Vmin).