# :MEASure:JITTer:NOISe:VECLosure:EYE

Noise VEC Commands

- :MEASure:JITTer:NOISe:VECLosure?
- :MEASure:JITTer:NOISe:VECLosure:EYE
- :MEASure:JITTer:NOISe:VECLosure:STATus?
- :MEASure:JITTer:NOISe:VECLosure:STATus:DETails?
- :MEASure:JITTer:NOISe:VECLosure:STATus:REASon?

## Command Syntax

    :MEASure:JITTerN:NOISe:VECLosure:EYE {EYE0}

Where N identifies one of four possible jitter/noise analyses {1:4}. For example, `JITTer4`.

## Query Syntax

    :MEASure:JITTerN:NOISe:VECLosure:EYE?

## Description

This command specifies the eye for which the measurement value is returned. Multiple eyes are present in PAM signals.