# :MEASure:VERTical:CPOWer:SOURce

Carrier Power Commands

- :MEASure:VERTical:CPOWer
- :MEASure:VERTical:CPOWer:AIMPedance
- :MEASure:VERTical:CPOWer:FAVorite
- :MEASure:VERTical:CPOWer:LOCation?
- :MEASure:VERTical:CPOWer:REGion
- :MEASure:VERTical:CPOWer:RIMPedance
- :MEASure:VERTical:CPOWer:SOURce
- :MEASure:VERTical:CPOWer:STATus?
- :MEASure:VERTical:CPOWer:STATus:DETails?
- :MEASure:VERTical:CPOWer:STATus:REASon?
- :MEASure:VERTical:CPOWer:UREFerence:STATe
- :MEASure:VERTical:CPOWer:UREFerence:VALue

## Command Syntax

    :MEASure:VERTical:CPOWer:SOURce <source_waveform>

Where <source_waveform> can be one of the following:

- `CHANnel{N}` — Where N identifies a specific channel in the form "<connection1-8>_<ch1-8>". With connection 1, the connection number part (that is, "1_") is optional, and you can simply use the channel number "<ch1-8>". For example, connection 4 channel 2 is `CHANnel4_2`.
- `DIFF{N}` — Where N identifies a specific differential waveform in the form "<connection1-8>_<ch1|ch3|ch5|ch7>". With connection 1, the connection number part (that is, "1_") is optional, and you can simply use the channel number "<ch1|ch3|ch5|ch7>". When two channels are paired to create a differential waveform and a common-mode waveform, the odd-numbered channel is used when specifying the waveform. For example, connection 5 differential waveform 3 (from the pairing of channels 3 and 4) is `DIFF5_3`.
- `CMODe{N}` — Where N identifies a specific common-mode waveform in the form "<connection1-8>_<ch1|ch3|ch5|ch7>". With connection 1, the connection number part (that is, "1_") is optional, and you can simply use the channel number "<ch1|ch3|ch5|ch7>". When two channels are paired to create a differential waveform and a common-mode waveform, the odd-numbered channel is used when specifying the waveform. For example, connection 5 common-mode waveform 3 (from the pairing of channels 3 and 4) is `CMODe5_3`.
- `FUNCtion{1:64}`
- `WMEMory{1:8}`

## Query Syntax

    :MEASure:VERTical:CPOWer:SOURce?

## Description

Selects the source waveform on which to perform the `:MEASure:VERTical:CPOWer` measurement.