# :MEASure:JITTer:NOISe:RNComp

Noise Setup Commands

- :MEASure:JITTer:NOISe:ANALysis
- :MEASure:JITTer:NOISe:ERNValue:LEVel
- :MEASure:JITTer:NOISe:MLOCation
- :MEASure:JITTer:NOISe:RNBandwidth
- :MEASure:JITTer:NOISe:RNComp
- :MEASure:JITTer:NOISe:RNCValue:LEVel
- :MEASure:JITTer:NOISe:RNSTabilize
- :MEASure:JITTer:NOISe:RNSValue:LEVel
- :MEASure:JITTer:NOISe:UNITs

## Command Syntax

    :MEASure:JITTerN:NOISe:RNComp {OFF | AUTomatic | CUSTom}

Where N identifies one of four possible jitter/noise analyses {1:4}. For example, `JITTer4`.

## Query Syntax

    :MEASure:JITTerN:NOISe:RNComp?

## Description

This command disable disables RN compensation (`OFF`), enables compensation for oscilloscope RN (`AUTomatic`), or enables user-defined values for RN compensation (`CUSTom`).

If there are known contributors to random noise, you can use RN Compensation to compensate or remove noise from the measurement results.

When `CUSTom` is selected, use the `:MEASure:JITTer:NOISe:RNCValue:LEVel` command to specify the appropriate RN compensation values for the symbol levels.