# :CMODe:DISPlay

:CMODe General Commands

- :CMODe:COLor
- :CMODe:CWINdow
- :CMODe:DISPlay
- :CMODe:PATTern:FILE:GCODe
- :CMODe:PATTern:FILE:NAME
- :CMODe:PATTern:FILE:RELoad
- :CMODe:PATTern:INVert
- :CMODe:PATTern:KPATtern
- :CMODe:PATTern:MODE
- :CMODe:SIGNal:TYPE
- :CMODe:SNOise:CALibrate
- :CMODe:SNOise:SNValue:LEVel{0:3}?
- :CMODe:STATus?
- :CMODe:UNAMe

## Command Syntax

    :CMODeN:DISPlay {ON | OFF | 1 | 0}

Where N identifies a specific common-mode waveform in the form "<connection1-8>_<ch1|ch3|ch5|ch7>". With connection 1, the connection number part (that is, "1_") is optional, and you can simply use the channel number "<ch1|ch3|ch5|ch7>". When two channels are paired to create a differential waveform and a common-mode waveform, the odd-numbered channel is used when specifying the waveform. For example, connection 5 common-mode waveform 3 (from the pairing of channels 3 and 4) is `CMODe5_3`.

## Query Syntax

    :CMODeN:DISPlay?

## Description

Turns the display of the specified common-mode waveform on or off. Use the `:CMODe:STATus?` command to determine if a common-mode waveform is available for display.

## Example

    :CMODe5_3:DISPlay ON