# :MEASure:EYE:PAM:PPAMplitude:STATus:REASon?

:PAM Pk-Pk Amplitude Commands

- :MEASure:EYE:PAM:PPAMplitude
- :MEASure:EYE:PAM:PPAMplitude:FAVorite
- :MEASure:EYE:PAM:PPAMplitude:LOCation?
- :MEASure:EYE:PAM:PPAMplitude:SOURce
- :MEASure:EYE:PAM:PPAMplitude:STATus?
- :MEASure:EYE:PAM:PPAMplitude:STATus:DETails?
- :MEASure:EYE:PAM:PPAMplitude:STATus:REASon?
- :MEASure:EYE:PAM:PPAMplitude:THRatio
- :MEASure:EYE:PAM:PPAMplitude:UNITs

## Query Syntax

    :MEASure:EYE:PAM:PPAMplitude:STATus:REASon?

## Query Response

Refer to the table "Common Reasons for INV or QUES Status".

## Description

Returns a string that explains the reason for a failed `:MEASure:EYE:PAM:PPAMplitude` measurement. If the measurement was successful, a null string is returned. Use the `:MEASure:EYE:PAM:PPAMplitude:STATus?` query to determine if the measurement has failed. Additional information about the failure may be available using the `:MEASure:EYE:PAM:PPAMplitude:STATus:DETails?` query.

## See Also

- Measurement Errors