# :TRIGger:PWIDth:MODE

:TRIGger Pulse Width Commands

- :TRIGger:PWIDth:MODE
- :TRIGger:PWIDth:POLarity
- :TRIGger:PWIDth:REND
- :TRIGger:PWIDth:RSTart
- :TRIGger:PWIDth:SOURce
- :TRIGger:PWIDth:WIDTh

## Command Syntax

    :TRIGger:PWIDth:MODE  {LTHan | GTPend | GTTimeout | RINSide | ROUTside}

## Query Syntax

    :TRIGger:PWIDth:MODE?

## Description

In the Pulse Width trigger mode (see `:TRIGger:MODE`), this command selects what kind of pulses will cause a trigger:

- `LTHan` — Pulses narrower than the specified `:TRIGger:PWIDth:WIDTh`. This is the same as the Glitch mode (see :TRIGger Glitch Commands).
- `GTPend` — Pulses wider than the specified `:TRIGger:PWIDth:WIDTh`, triggering when the pulse ends.
- `GTTimeout` — Pulses wider than the specified `:TRIGger:PWIDth:WIDTh`, triggering when the width is exceeded. This is the same as the Timeout mode (see :TRIGger Timeout Commands).
- `RINSide` — Pulses within the range specified by the `:TRIGger:PWIDth:RSTart` and `:TRIGger:PWIDth:REND` values.
- `ROUTside` — Pulses outside the range specified by the `:TRIGger:PWIDth:RSTart` and `:TRIGger:PWIDth:REND` values.