# :MEASure:EYE:PAM:ESKew:EYE

Eye Skews Commands

- :MEASure:EYE:PAM:ESKew
- :MEASure:EYE:PAM:ESKew:EYE
- :MEASure:EYE:PAM:ESKew:FAVorite
- :MEASure:EYE:PAM:ESKew:LOCation?
- :MEASure:EYE:PAM:ESKew:SOURce
- :MEASure:EYE:PAM:ESKew:STATus?
- :MEASure:EYE:PAM:ESKew:STATus:DETails?
- :MEASure:EYE:PAM:ESKew:STATus:REASon?

## Command Syntax

    :MEASure:EYE:PAM:ESKew:EYE {EYE0 | EYE1 | EYE2}

## Query Syntax

    :MEASure:EYE:PAM:ESKew:EYE?

## Description

This command allows you to select an eye on PAM signals on which to perform the `:MEASure:EYE:PAM:ESKew` measurement. For NRZ signals, the argument `EYE0` is automatically selected and cannot be changed. If you experience difficulties measuring a PAM signal, confirm that the signal-type setting is set appropriately using the `:CHANnel:SIGNal:TYPE` command.

NRZ Waveform
PAM3 Waveform
PAM4 Waveform