# :MEASure:VERTical:VRMS:UREFerence:VALue

Vrms Commands

- :MEASure:VERTical:VRMS
- :MEASure:VERTical:VRMS:AREA
- :MEASure:VERTical:VRMS:EDIRection
- :MEASure:VERTical:VRMS:FAVorite
- :MEASure:VERTical:VRMS:LOCation?
- :MEASure:VERTical:VRMS:REGion
- :MEASure:VERTical:VRMS:SOURce
- :MEASure:VERTical:VRMS:STATus?
- :MEASure:VERTical:VRMS:STATus:DETails?
- :MEASure:VERTical:VRMS:STATus:REASon?
- :MEASure:VERTical:VRMS:TYPE
- :MEASure:VERTical:VRMS:UREFerence:STATe
- :MEASure:VERTical:VRMS:UREFerence:VALue

## Command Syntax

    :MEASure:VERTical:VRMS:UREFerence:VALue <time_location>

<time_location> is a double.

## Query Syntax

    :MEASure:VERTical:VRMS:UREFerence:VALue?

## Description

When a user-defined horizontal reference location is enabled (see `:MEASure:VERTical:VRMS:UREFerence:STATe`), this command specifies its time location with respect to the trigger (t = 0) location.