# :MEASure:USER:USER{N}:UREFerence:STATe

User-Defined Waveform Measurement Commands

- :MEASure:USER:USER{N}
- :MEASure:USER:USER{N}:ABBReviation?
- :MEASure:USER:USER{N}:CFILe
- :MEASure:USER:USER{N}:CFILe:CLEar
- :MEASure:USER:USER{N}:CFILe:RELoad
- :MEASure:USER:USER{N}:CFLoaded?
- :MEASure:USER:USER{N}:COMMents?
- :MEASure:USER:USER{N}:FAVorite
- :MEASure:USER:USER{N}:LOCation?
- :MEASure:USER:USER{N}:LSTatus?
- :MEASure:USER:USER{N}:LSTatus:REASon?
- :MEASure:USER:USER{N}:NAME?
- :MEASure:USER:USER{N}:REGion
- :MEASure:USER:USER{N}:SOURce{1:2}
- :MEASure:USER:USER{N}:STATus?
- :MEASure:USER:USER{N}:STATus:DETails?
- :MEASure:USER:USER{N}:STATus:REASon?
- :MEASure:USER:USER{N}:UREFerence:STATe
- :MEASure:USER:USER{N}:UREFerence:VALue

## Command Syntax

    :MEASure:USER:USER{1:8}:UREFerence:STATe {ON | OFF | 1 | 0}

## Query Syntax

    :MEASure:USER:USER{1:8}:UREFerence:STATe?

## Query Response

    {1 | 0}

## Description

Enables or disables a user-defined horizontal reference location near which a one-measurement-per-acquisition measurement is made.

When a user-defined horizontal reference location is enabled, the `:MEASure:USER:USER{N}:UREFerence:VALue` command specifies its time location with respect to the trigger (t = 0) location.