# :MEASure:EYE:PAM:OVERshoot:THRatio

PAM Overshoot Commands

- :MEASure:EYE:PAM:OVERshoot
- :MEASure:EYE:PAM:OVERshoot:FAVorite
- :MEASure:EYE:PAM:OVERshoot:LOCation?
- :MEASure:EYE:PAM:OVERshoot:SOURce
- :MEASure:EYE:PAM:OVERshoot:STATus?
- :MEASure:EYE:PAM:OVERshoot:STATus:DETails?
- :MEASure:EYE:PAM:OVERshoot:STATus:REASon?
- :MEASure:EYE:PAM:OVERshoot:THRatio

## Command Syntax

    :MEASure:EYE:PAM:OVERshoot:THRatio <hit_ratio>

<hit_ratio> is a double.

## Query Syntax

    :MEASure:EYE:PAM:OVERshoot:THRatio?

## Description

Sets the hit ratio for the PAM overshoot measurement (`:MEASure:EYE:PAM:OVERshoot`. The default hit ratio is 1e-2 which is called out in the IEEE 802.3cu standard. The minimum value is 0.0. The maximum value is 0.1.