# :MEASure:JITTer:NOISe:MLOCation

Noise Setup Commands

- :MEASure:JITTer:NOISe:ANALysis
- :MEASure:JITTer:NOISe:ERNValue:LEVel
- :MEASure:JITTer:NOISe:MLOCation
- :MEASure:JITTer:NOISe:RNBandwidth
- :MEASure:JITTer:NOISe:RNComp
- :MEASure:JITTer:NOISe:RNCValue:LEVel
- :MEASure:JITTer:NOISe:RNSTabilize
- :MEASure:JITTer:NOISe:RNSValue:LEVel
- :MEASure:JITTer:NOISe:UNITs

## Command Syntax

    :MEASure:JITTerN:NOISe:MLOCation <pct_of_bit>

Where N identifies one of four possible jitter/noise analyses {1:4}. For example, `JITTer4`.

<pct_of_bit> is a double.

## Query Syntax

    :MEASure:JITTerN:NOISe:MLOCation?

## Description

This command specifies the measurement location within the bit where 0% is the beginning of the bit, 50% is the middle of the bit, and 100% is the end of the bit.

You can specify a location value from 5% to 95%.