# :CGMemory:XPOSition?

:CGMemory Scaling Commands

- :CGMemory:XLEFt?
- :CGMemory:XPOSition?
- :CGMemory:XREFerence?
- :CGMemory:XRIGht?
- :CGMemory:XSCale?
- :CGMemory:XUNits?
- :CGMemory:YBOTtom?
- :CGMemory:YOFFset?
- :CGMemory:YRANge?
- :CGMemory:YSCale?
- :CGMemory:YTOP?
- :CGMemory:YUNits?

## Query Syntax

    :CGMemoryN:XPOSition?

Where N identifies one of eight color grade memories. For example, the color grade memory 2 would be identified as :CGMemory2.

## Description

Queries the horizontal time position which is stored for the waveform in eye-memory. It may or may not be the same as Infiniium's current setting. The horizontal position is the time delay relative to the trigger event, which is referenced to the display's left edge or center (`:CGMemory:XREFerence?`). The horizontal reference and position of the original waveform was set with the `:TIMebase:REFerence` and `:TIMebase:POSition` commands.