# :LTESt:MEASure:SIMage:INVert

:LTESt Measurement Screen Image Commands

- :LTESt:MEASure:SIMage:FNAMe
- :LTESt:MEASure:SIMage:FNAMe:AUPDate
- :LTESt:MEASure:SIMage:FNAMe:USTandard
- :LTESt:MEASure:SIMage:FTYPe?
- :LTESt:MEASure:SIMage:IMETadata
- :LTESt:MEASure:SIMage:INVert
- :LTESt:MEASure:SIMage:MONochrome
- :LTESt:MEASure:SIMage:SINClude
- :LTESt:MEASure:SIMage:STATe
- :LTESt:MEASure:SIMage:WINDow

## Command Syntax

    :LTESt:MEASure:SIMage:INVert {ON | OFF | 1 | 0}

## Query Syntax

    :LTESt:MEASure:SIMage:INVert?

## Query Response

    {1 | 0}

## Description

Turns on and off the inversion of the graticule area's background color when reporting a screen capture for a measurement limit test. When on, an inverted image will be captured and saved into a file by the `:LTESt:ACQuire:SIMage:FNAMe` command. The entire application window is saved with the graticule black upon a white background. The waveform colors remain unchanged. When printing a hard copy of the waveform, combine this command with the `:LTESt:MEASure:SIMage:WINDow` command (graticule only) to save ink or toner. Use the `:LTESt:MEASure:SIMage:STATe` command to enable and disable screen-capture reporting.