# :NETWorks:TRACe:XUNits?

:NETWorks:TRACe Scaling Commands

- :NETWorks:TRACe:XLEFt?
- :NETWorks:TRACe:XPOSition?
- :NETWorks:TRACe:XREFerence?
- :NETWorks:TRACe:XRIGht?
- :NETWorks:TRACe:XSCale?
- :NETWorks:TRACe:XUNits?
- :NETWorks:TRACe:YBOTtom?
- :NETWorks:TRACe:YOFFset?
- :NETWorks:TRACe:YRANge?
- :NETWorks:TRACe:YSCale?
- :NETWorks:TRACe:YTOP?
- :NETWorks:TRACe:YUNits?

## Query Syntax

    :NETWorks:TRACeN:XUNits?

Where N identifies a specific trace and must be selected from 1 to 128 {1:128}.

## Query Response

    {HERT}

## Description

Queries the X-axis units-of-measurement for the indicated S-parameter trace. The units for S-parameters is Hertz which is indicated with the returned `HERT` string.

Returned Values with Displayed Content Window Graph
Returned String | X-Axis Units | Content Window Graphs
--- | --- | ---
S-Parameters
HERT | Hertz | Freq-Mag
Phase
GrpDelay