# :FUNCtion:PARameters:CTLequalizer:BANDwidth

CTLE Parameters Commands

- :FUNCtion:PARameters:CTLequalizer:ACGain
- :FUNCtion:PARameters:CTLequalizer:BANDwidth
- :FUNCtion:PARameters:CTLequalizer:BWMode
- :FUNCtion:PARameters:CTLequalizer:DBACgain
- :FUNCtion:PARameters:CTLequalizer:DBGain
- :FUNCtion:PARameters:CTLequalizer:DEFinition
- :FUNCtion:PARameters:CTLequalizer:FZP
- :FUNCtion:PARameters:CTLequalizer:GAIN
- :FUNCtion:PARameters:CTLequalizer:GDC
- :FUNCtion:PARameters:CTLequalizer:IMPulse
- :FUNCtion:PARameters:CTLequalizer:POLE
- :FUNCtion:PARameters:CTLequalizer:PRESets
- :FUNCtion:PARameters:CTLequalizer:PRESets:SELections?
- :FUNCtion:PARameters:CTLequalizer:STEP
- :FUNCtion:PARameters:CTLequalizer:TFUNction
- :FUNCtion:PARameters:CTLequalizer:ZERO

## Command Syntax

    :FUNCtionN:PARameters:CTLequalizer:BANDwidth <bandwidth>

<bandwidth> is a double.

Where N identifies one of up to 64 possible operators {1:64} that can be defined as part of a math function. The operators are numbered in the order that they were originally added to the function.

## Query Syntax

    :FUNCtionN:PARameters:CTLequalizer:BANDwidth?

## Description

In the `CUSTom` linear Bandwidth Mode (`:FUNCtion:PARameters:CTLequalizer:BWMode`), this command specifies the linear bandwidth, in Hertz, of a Continuous TimeLinear Equalizer operator (CTLE) (`:FUNCtion:FOPerator`).

## Example Command Sequence

    :FUNCtion2:FOPerator CTLE
    :FUNCtion2:PARameters:CTLequalizer:BWMode CUSTom
    :FUNCtion2:PARameters:CTLequalizer:BANDwidth 8.0E9
    :FUNCtion2:DISPlay ON
    *OPC?
    …  //  Your code to synchronize execution timing.