# :LTESt:MEASure:SWAVeform:DIFF{N}:WMEMory

:LTESt Measurement Waveform Commands

- :LTESt:MEASure:SWAVeform:CHANnel{N}:FNAMe
- :LTESt:MEASure:SWAVeform:CHANnel:FTYPe
- :LTESt:MEASure:SWAVeform:CHANnel{N}:STATe
- :LTESt:MEASure:SWAVeform:CHANnel{N}:WMEMory
- :LTESt:MEASure:SWAVeform:CMODe{N}:FNAMe
- :LTESt:MEASure:SWAVeform:CMODe:FTYPe
- :LTESt:MEASure:SWAVeform:CMODe{N}:STATe
- :LTESt:MEASure:SWAVeform:CMODe{N}:WMEMory
- :LTESt:MEASure:SWAVeform:DIFF{N}:FNAMe
- :LTESt:MEASure:SWAVeform:DIFF:FTYPe
- :LTESt:MEASure:SWAVeform:DIFF{N}:STATe
- :LTESt:MEASure:SWAVeform:DIFF{N}:WMEMory
- :LTESt:MEASure:SWAVeform:FUNCtion{N}:FNAMe
- :LTESt:MEASure:SWAVeform:FUNCtion{N}:STATe
- :LTESt:MEASure:SWAVeform:FUNCtion{N}:WMEMory
- :LTESt:MEASure:SWAVeform:RESet

## Command Syntax

    :LTESt:MEASure:SWAVeform:DIFF{N}:WMEMory WMEMory{1:8}

{N} identifies the differential waveform, which must be selected from "<connection1-8>_<ch1,3,5,7>". For example, the differential waveform of connection 4 channels 1 and 2 would be identified as DIFF4_1.

## Query Syntax

    :LTESt:MEASure:SWAVeform:DIFF{N}:WMEMory?

## Description

Upon completion of an measurement limit test, selects a waveform memory as a destination to save a differential waveform. Use the `:LTESt:MEASure:SWAVeform:DIFF{N}:STATe` command to enable and disable waveform reporting for the channel. Use the `:LTESt:MEASure:MLIMit:STATe` command to turn off the measurement limit test