# :LTESt:LLINe:SWAVeform:CMODe{N}:STATe

:LTESt Limit Line Commands

- :LTESt:LLINe:TEST{N}:MODE
- :LTESt:LLINe:TEST{N}:STATe
- :LTESt:LLINe:SIMage:FNAMe
- :LTESt:LLINe:SIMage:FNAMe:AUPDate
- :LTESt:LLINe:SIMage:FNAMe:USTandard
- :LTESt:LLINe:SIMage:FTYPe?
- :LTESt:LLINe:SIMage:IMETadata
- :LTESt:LLINe:SIMage:INVert
- :LTESt:LLINe:SIMage:MONochrome
- :LTESt:LLINe:SIMage:SAVE
- :LTESt:LLINe:SIMage:SINClude
- :LTESt:LLINe:SIMage:STATe
- :LTESt:LLINe:SIMage:WINDow
- :LTESt:LLINe:SSUMmary:FNAMe
- :LTESt:LLINe:SSUMmary:STATe
- :LTESt:LLINe:SWAVeform:CHANnel{N}:FNAMe
- :LTESt:LLINe:SWAVeform:CHANnel:FTYPe
- :LTESt:LLINe:SWAVeform:CHANnel{N}:STATe
- :LTESt:LLINe:SWAVeform:CHANnel{N}:WMEMory
- :LTESt:LLINe:SWAVeform:CMODe{N}:FNAMe
- :LTESt:LLINe:SWAVeform:CMODe:FTYPe
- :LTESt:LLINe:SWAVeform:CMODe{N}:STATe
- :LTESt:LLINe:SWAVeform:CMODe{N}:WMEMory
- :LTESt:LLINe:SWAVeform:DIFF{N}:FNAMe
- :LTESt:LLINe:SWAVeform:DIFF:FTYPe
- :LTESt:LLINe:SWAVeform:DIFF{N}:STATe
- :LTESt:LLINe:SWAVeform:DIFF{N}:WMEMory
- :LTESt:LLINe:SWAVeform:FUNCtion{N}:FNAMe
- :LTESt:LLINe:SWAVeform:FUNCtion{N}:STATe
- :LTESt:LLINe:SWAVeform:FUNCtion{N}:WMEMory
- :LTESt:LLINe:SWAVeform:RESet

## Command Syntax

    :LTESt:LLINe:SWAVeform:CMODeN:STATe {DISK | MEMory | OFF}

Where N identifies a specific common-mode waveform in the form "<connection1-8>_<ch1|ch3|ch5|ch7>". With connection 1, the connection number part (that is, "1_") is optional, and you can simply use the channel number "<ch1|ch3|ch5|ch7>". When two channels are paired to create a differential waveform and a common-mode waveform, the odd-numbered channel is used when specifying the waveform. For example, connection 5 common-mode waveform 3 (from the pairing of channels 3 and 4) is `CMODe5_3`.

## Query Syntax

    :LTESt:LLINe:SWAVeform:CMODeN:STATe?

## Description

Specifies the reporting action for the selected common-mode waveforms upon completion of limit testing for a limit line test. Use the command argument to select or turn off the reporting action. To disable the reporting action of all channel, common-mode, differential, and function waveforms, use the `:LTESt:LLINe:SWAVeform:RESet` command.

To turn on limit testing for a limit line test, use the `:LTESt:LLINe:TEST{N}:STATe` command.

Command Arguments
Argument | Description
--- | ---
DISK | Saves the waveform to a file (.h5) in the `%USER_DATA_DIR%\Limit Lines` folder. Use the `:LTESt:LLINe:SWAVeform:CMODe{N}:FNAMe` command to specify the file name.
MEMory | Saves the waveform to a memory location. Use the `:LTESt:LLINe:SWAVeform:CMODe{N}:WMEMory` command to specify the memory location.
OFF | Turns off the saving of a common-mode waveform.