# :MEASure:EYE:JITTer:FORMat

Eye Jitter Commands

- :MEASure:EYE:JITTer
- :MEASure:EYE:JITTer:DEFine:SIGNal
- :MEASure:EYE:JITTer:DEFine:SIGNal:AUTodetect
- :MEASure:EYE:JITTer:DEFine:UNITs
- :MEASure:EYE:JITTer:FAVorite
- :MEASure:EYE:JITTer:FORMat
- :MEASure:EYE:JITTer:LOCation?
- :MEASure:EYE:JITTer:SOURce
- :MEASure:EYE:JITTer:STATus?
- :MEASure:EYE:JITTer:STATus:DETails?
- :MEASure:EYE:JITTer:STATus:REASon?
- :MEASure:EYE:JITTer:UNITs

## Command Syntax

    :MEASure:EYE:JITTer:FORMat  {PP | RMS}

## Query Syntax

    :MEASure:EYE:JITTer:FORMat?

## Description

Selects the format of the :JITTer measurement: peak-to-peak or RMS. Set the format before turning the measurement on. Jitterp-p is equal to the full width of the histogram at the eye crossing point.

JitterRMS is defined as 1σ (standard deviation) of the crossing point histogram.