# :MEASure:JITTer:JITTer:TFILter:STOP

Jitter/Noise Advanced Setup Commands

- :MEASure:JITTer:JITTer:TFILter:DFACtor
- :MEASure:JITTer:JITTer:TFILter:SHAPe
- :MEASure:JITTer:JITTer:TFILter:STARt
- :MEASure:JITTer:JITTer:TFILter:STOP
- :MEASure:JITTer:JITTer:TFILter:TYPE
- :MEASure:JITTer:TFILter:STATe

## Command Syntax

    :MEASure:JITTerN:JITTer:TFILter:STOP <frequency>

Where N identifies one of four possible jitter/noise analyses {1:4}. For example, `JITTer4`.

<frequency> is a double.

## Query Syntax

    :MEASure:JITTerN:JITTer:TFILter:STOP?

## Description

This command lets you specify the TIE filter's stop frequency. Frequencies above this value are filtered out of the TIE measurement.