# :CGMemory:UNAMe

:CGMemory General Commands

- :CGMemory:CLEar
- :CGMemory:COLor
- :CGMemory:CWINdow
- :CGMemory:DISPlay
- :CGMemory:DSTatus?
- :CGMemory:DSTatus:REASon?
- :CGMemory:PERSistence
- :CGMemory:SIGNal:TYPE
- :CGMemory:STATus?
- :CGMemory:UNAMe
- :CGMemory:UNAMe:UFName

## Command Syntax

    :CGMemoryN:UNAMe <string>

Where N identifies one of eight color grade memories. For example, the color grade memory 2 would be identified as :CGMemory2.

## Query Syntax

    :CGMemoryN:UNAMe?

## Description

Assigns a custom user name to an eye-memory waveform. User names are helpful because they identify what a waveform represents rather than the oscilloscope's input channel. For example, you could assign user name "DUT Output" to the memory 2 waveform. User names can be 25 characters or less and are displayed on the screen and on screen captures. To remove a custom user name, re-create it using an empty string. To assign the user name to the name of the gray-scale and color-grade database waveform file that was imported into color grade memory, use the `:CGMemory:UNAMe:UFName` command.

Custom user names can by created for other waveforms using the following commands:

- `:CHANnel:UNAMe`
- `:CMODe:UNAMe`
- `:DIFF:UNAMe`
- `:FUNCtion:UNAMe`
- `:WMEMory:UNAMe`

## Example Command Sequence

    :CGMemory2:UNAMe "DUT Output"