# :MEASure:EYE:CONTour:RJSValue:EYE

Eye Contour Configuration Commands

- Eye Contour Configuration Commands
- :MEASure:EYE:CONTour:BERates
- :MEASure:EYE:CONTour:DISPlay
- :MEASure:EYE:CONTour:PSPec
- :MEASure:EYE:CONTour:RJSTabilize
- :MEASure:EYE:CONTour:RJSValue:EYE
- :MEASure:EYE:CONTour:RNSTabilize
- :MEASure:EYE:CONTour:RNSValue:LEVel
- :MEASure:EYE:CONTour:SOURce

## Command Syntax

    :MEASure:EYE:CONTourN:RJSValue:EYE{0:2} <random_jitter>

Where N identifies a group of contour lines and must be {1:16}. <random_jitter> is a double.

## Query Syntax

    :MEASure:EYE:CONTourN:RJSValue:EYE{0|1|2}?

## Description

For Random Jitter (RJ) stabilization, sets the value of RJ for the selected eye of an eye-contour group. To measure the RJ, measure the RJ while using a signal that has a short pattern. Or, measure the RJ using a separate instrument, such as a spectrum analyzer. Use the `:MEASure:EYE:CONTour:RJSTabilize` command to turn on or off the use of RJ stabilization.

Command | Description
--- | ---
:EYEl2 | Applies to eye 2/3. |
:EYE1 (or :EYE) | Applies to eye 1/2.
:EYE0 | Applies to eye 0/1.